Release Note

Memory Switch Setting Utility for Windows (MSWUTL)

for TM Series

Version 2.31 (Def Ver. 2.31.03)

Issue Date : February. 22, 2006

1. Outline

> MSWUTL has following features.

> - Supported TM-H5000II, TM-H5200, TM-H6000, TM-H6000II, TM-H6000III, TM-J2000, TM-J2100, TM-J7000, TM-J7100, TM-J7500, TM-J7600, TM-J9000, TM-J9100, TM-L90, TM-L90 Peeler, TM-P60, TM-P60 Peeler, TM-T260F, TM-H3000R, TM-T81F, TM-T86L, TM-T87L, TM-T88IV, TM-T90, TM-U120, TM-U220, TM-U220BM, TM-U675.
> - Can execute communication test.
> - Can set memory switches. (Memory Switch / Customize value etc)
> - Included License Agreement screen.

2. Contents of this release version

> Memory Switch Setting Utility for TM series (MSWUTL)

> > MSW23103us.exe (Self-extracting file) included Setup files.
> > And included files are

> > - User's Manual
> > - Definition files Version 2.31.03 of support models (See Section 3)
> > - Release note (MSWUTLRelNote0602E.htm)
> > - USB Device Driver Ver.2.00 (Zipped file TMUSB200a.zip)

3. Supports

> Environment

> > Operating System

> > - Windows 2000 SP4

> > - Windows XP SP2

> > Disk Space

> > - 2 MB or more of free space

> > Communication Ports

> > - COMx
> >   * But, XON/XOFF handshaking is not supported. Please change handshaking of TM Printer to DTR/DSR handshaking when you use this utility.
> >   * Specify Serial I/F when you use Bluetooth I/F. But, If you execute function of Firmware update, Backup and Restore, please specify the most faster baud-rate of the products.
> > - LPT1
> >   * On Windows 2000 or Windows XP, you cannot use LPT Port when other printer driver (Terminal Printer etc.) was mounted on same port. Please release port for this utility when you use this utility.
> > - USB
> >   * Installation of the USB driver is necessary when you use the USB I/F.
> >   * Use USB driver which is included in OPOS ADK or APD. Use the USB driver which is included in this utility only if you don't use OPOS ADK and APD.
> >   * You can use only one USB device at a time.
> > - Ethernet
> >   * Specify the IP Address which is set to the TM Printer.
> >   * Specify Ethernet I/F when you use 802.11b Wireless LAN I/F.

> Support Models

> Model Name | Definition File Name (Def File Version) | TMSSUTL for TM | TMSSUTL for EUBA
> Setup | Web Update | Setup | Web Update
> English | Japanese | USA | Europe | Asia | Japan | USA | Europe | Asia | Japan
> TM-H5000II *5 | TM-H5k2.def (2.00.00) | Inc. | Inc. | A00 | A00 | A00 | A00 | - | - | - | - | -
> TM-H6000 *5 | TM-H6k.def (2.00.00) | Inc. | Inc. | A00 | A00 | A00 | A00 | - | - | - | - | -
> TM-H6000II *5 | TM-H6k2.def (2.20.00) | Inc. | Inc. | C00 | C00 | C00 | C00 | - | - | - | - | -
> TM-H6000II with Scanner *5 | TM-H6k2s.def (2.10.01) | Inc. | - | B01 | B01 | B01 | - | - | - | - | - | -
> TM-H6000II with Photo ID *5 | TM-H6k2c.def (2.10.01) | Inc. | - | B01 | B01 | B01 | - | - | - | - | - | -
> TM-H6000II Validation *5 | TM-H6k2v.def (2.10.01) | Inc. | - | B01 | B01 | B01 | - | - | - | - | - | -
> TM-H6000III *5 Updated | TM-H6k3.def (2.31.02) | Inc. | Inc. | D102 | D102 | D102 | D102 | - | - | - | - | -
> TM-H6000III with Scanner *5 New | TM-H6k3s.def (2.31.03) | Inc. | - | D103 | D103 | D103 | - | - | - | - | - | -
> TM-H6000III with Photo ID *5 New | TM-H6k3c.def (2.31.03) | Inc. | - | D103 | D103 | D103 | - | - | - | - | - | -
> TM-H6000III Validation *5 New | TM-H6k3v.def (2.31.03) | Inc. | - | D103 | D103 | D103 | - | - | - | - | - | -
> TM-J2000 | TM-J2k.def (2.20.00) | Inc. | Inc. | C00 | C00 | C00 | C00 | - | - | - | - | -
> TM-J2100 | TM-J2t.def (2.00.00) | Inc. | Inc. | C00 | C00 | C00 | C00 | - | - | - | - | -
> TM-J7000 | TM-J7k.def (2.20.00) | Inc. | - | C00 | C00 | C00 | - | - | - | - | - | -
> TM-J7100 | TM-J7t.def (2.00.00) | Inc. | - | A00 | A00 | A00 | - | - | - | - | - | -
> TM-J7500 | TM-J75.def (2.20.00) | Inc. | - | C00 | C00 | C00 | - | - | - | - | - | -
> TM-J7600 | TM-J76.def (2.00.00) | Inc. | - | A00 | A00 | A00 | - | - | - | - | - | -
> TM-J9000 | TM-J9k.def (2.10.02) | Inc. | - | B02 | B02 | B02 | - | - | - | - | - | -
> TM-J9100 | TM-J9t.def (2.10.02) | Inc. | - | B02 | B02 | B02 | - | - | - | - | - | -
> TM-P60 (802.11b) | TM-P60.def (2.10.00) | Inc. | Inc. | B00 | B00 | B00 | B00 | - | - | - | - | -
> TM-P60 (bluetooth) | TM-P60BT.def (2.10.00) | - | - | B00 | - | - | B00 | - | - | - | - | -
> TM-P60 peeler | TM-P60p.def (2.20.00) | Inc. | - | C00 | C00 | C00 | - | - | - | - | - | -
> TM-T90 | TM-T90.def (2.10.00) | Inc. | Inc. | B01 | B01 | B01 | B01 | - | - | - | - | -
> TM-T88IV | TM-T884.def (2.30.00) | Inc. | - | B01 | B01 | B01 | - | - | - | - | - | -
> TM-T90 *4 (TM-T88II Compatible Mode) | T90-T88c.def (2.10.00) | Inc. | Inc. | B01 | B01 | B01 | B01 | - | - | - | - | -
> TM-L90 | TM-L90.def (2.20.00) | Inc. | Inc. | C00 | C00 | C00 | C00 | - | - | - | - | -
> TM-L90 Peeler | TM-L90p.def (2.20.00) | Inc. | Inc. | C00 | C00 | C00 | C00 | - | - | - | - | -
> TM-U220 *5 | Tm-u220.def (2.20.00) | Inc. | Inc. | C00 | C00 | C00 | C00 | - | - | - | - | -
> TM-U675 *5 | TM-U675.def (2.00.00) | Inc. | Inc. | A00 | A00 | A00 | A00 | - | - | - | - | -
> TM-H5200 *5 | Tm-h52.def (2.00.00) | - | - | A00 | - | - | - | - | - | - | - | -
> TM-U120 *5 Updated | Tm-u120.def (2.31.00) | - | - | - | - | D100 | - | - | - | - | - | -
> TM-U220 with BM *5 | Tm-u220BM.def (2.20.00) | - | - | - | - | C00 | - | - | - | - | - | -
> TM-H3000R | TM-H3kr.def (2.00.00) | Inc. | - | A00 | A00 | A00 | - | - | - | - | - | -
> TM-T260F | TM-T260F.def (2.00.00) | - | - | - | A00 | - | - | - | - | - | - | -
> TM-T70 New | TM-T70.def (2.31.00) | - | Inc. | - | - | - | D100 | - | - | - | - | -
> TM-T81F Italy New | TM-T81F_I.def (2.31.00) | - | - | - | D100 | - | - | - | - | - | - | -
> TM-T86L | TM-T86L.def (2.20.00) | - | - | - | - | C00 | - | - | - | - | - | -
> TM-T87L | TM-T87L.def (2.20.00) | - | - | - | - | C00 | - | - | - | - | - | -
> BA-T500 | BA-M5xx.def (2.00.00) | - | - | - | - | - | - | Inc. | A00 | A00 | A00 | A00
> BA-T500 USB | BA-uM5x.def (2.00.00) | - | - | - | - | - | - | Inc. | A00 | A00 | A00 | A00
> EU-T300 | EU-T3xxxx.def (2.01.02) | - | - | - | - | - | - | Inc. | A102 | A102 | A102 | A102
> EU-T300 USB | EU-T3xxu.def (2.01.02) | - | - | - | - | - | - | Inc. | A102 | A102 | A102 | A102
> EU-T400 | EU-T4xx.def (2.00.00) | - | - | - | - | - | - | Inc. | A00 | A00 | A00 | A00
> EU-T500 | EU-T5xx.def (2.00.00) | - | - | - | - | - | - | Inc. | A00 | A00 | A00 | A00

> > > *1 : Use this definition file when MSW8-7(TM-T88II compatible mode) of TM-T90 is ON.
> > > *2 : You have to set the DSW2-8 to ON if you use the UB-U01/02(II).
> > > A**: Def file Ver.2.00.** will be added when webupdate is executed.
> > > A1**: Def file Ver.2.01.** will be added when webupdate is executed.
> > > B**: Def file Ver.2.10.** will be added when webupdate is executed.
> > > C**: Def file Ver.2.20.** will be added when webupdate is executed.
> > > D**: Def file Ver.2.30.** will be added when webupdate is executed.
> > > D1**: Def file Ver.2.31.** will be added when webupdate is executed.

> Support Function (Supt. : Supported / no: Not supported)

Function | Outline of function |  | Model
T90 T88c | T88IV T70 | T81F | P60 | L90 | H6k* | J2k | J7* J9* | C100 | T8*L | H5k2 H52 | T260F | H6k U675 | U220 U120 | H3kr | BA | EU
Communication Test |  |  | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt.
Printer Status | Memory Switch *1 | Indicate or change for Memory switch settings |  | Supt. | no | Supt. | Supt. | Supt. | Supt. | Supt. | no | no | Supt. | no | no | Supt. | Supt. | no | Supt. | Supt.
Dip Switch *1 | Indicate for Dip switch settings |  | Supt. | no | no | no | Supt. | no | Supt. | Supt. | no | no | no | no | no | no | no | no | no
Communication Condition *1 | Indicate or change for communication condition of memory switch |  | Supt. | Supt. | Supt. | Supt. | Supt. | no | Supt. | Supt. | no | no | no | no | no | Supt. | no | no | no
User NV / User NVG | Indicate capacity for User-NV and for User NVG |  | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | no | no | no | no | no | no | no | no | no
Customize Value *1 | Indicate or change for customize value |  | Supt. | Supt. | no | Supt. | Supt. | Supt. | Supt. | Supt. | no | no | no | Supt. | Supt. | Supt. | no | no | no
Reset able Maintenance Counter *1 | Indicate or reset for reset able maintenance counter |  | Supt. | Supt. | no | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | Supt. | no | Supt. | no | Supt. | no | Supt.
Paper Layout settings *1 | Indicate or change paper layout settings |  | no | no | no | no | Supt. | no | no | no | no | no | no | no | no | no | no | no | no
Head Nozzle Check | Print pattern for Head nozzle check |  | no | no | no | no | no | no | Supt. | no | no | no | no | no | no | no | no | no | no
Paper Layout Setting | Execute when you want to change the paper type |  | no | no | no | no | Supt. | no | no | no | no | no | no | no | no | no | no | no | no

> > *1 : Please refer to the specification, for values which it can read or it can set
> > *2 : Selectable for output sheet (Receipt and SLIP).

4. History

Release Version (Issue Date) | History

Ver.2.31.03 (February 22, 2006)

* Newly supported the TM-H6000III with Scanner / Photo ID / Validation.

Ver.2.31.02 (February 22, 2006)

* Updated the TM-H6000III.

Ver.2.31.00 (January 27, 2006)

* Fixed the problem that the communication condition of printer status can not be got.
* Modified the Model Definition file(TM-u120.def) to add the MSW for TM-U120.
* Newly supported the TM-T81F for Italy.

Ver.2.30.00 (December. 21, 2005)

* Newly supported the TM-T88IV.

Ver.2.20.00 (August. 31, 2005)

* TM-U120: Newly supported.
* Windows 2000 SP4 and Windows XP SP2 are supported.
* Fixed the problem that the communication error occurs when the printer is reset with USB/IF under Windows XP environment.

Ver.2.10.02 (August. 31, 2005)

* Supported the TM-P60 with Peeler.
* Updated the TM-J9000, TM-J9100.

Ver.2.10.01 (June. 30, 2005)

* Supported the TM-H6000III.
* Added the TM-P60(Bluetooth) to the Web Update for America area.
* Modified the problem of Model definition file for TM-T90, TM-H6000II, TM-H6000II with Image Scanner, TM-H6000II with Image Scanner (Photo ID), TM-H6000II Validation Model.

Ver.2.10 (Mar. 18, 2005)

* Fixed the problem of the Printer Status function.
* Supported the Windows XP.

Ver.2.01 (Nov. 5, 2004)

* Supported the TM-L90 Peeler.

Ver.2.00 (Sep 10, 2004)
* Changed the user interface.
* Supported the Ethernet I/F.
* Supported the Web Update function.
* Supported the TM-J9000, J9100.
* Supported the TM-C100.
Ver.1.37 (Mar 24, 2004)
* Supported the TM-P60.
* Modified the DEF file for TM-T90. (Added the MSW8-3 function)
Ver.1.36 (Oct 1, 2003)
* Supported the TM-H6000II with Image Scanner (Photo ID) Model and TM-H6000II Validation Model.
* Modified the DEF file for TM-L90. (Added the MSW8-3 function)
Ver.1.35 (May 14, 2003)
*Supported the TM-U220.
*Modified the DEF file for TM-T90. (Added the MSW8-3 function)
Ver.1.34 (February 26 2003)
Add Support Model (TM-J7500, TM-J7600)
Def file version is 1.32.
Ver.1.32 (July 10 2002)
Add Support Model (TM-J7000, TM-J7100, TM-H3000R)
Supported USB I/F.
Def file version is 1.32.
Ver.1.22 (December 26 2001)
New Release
Def file version is 1.22.